Version: 0.0.8

Release date:2019/3/11

Change:

1. Merge “Farfield” hotword model into firmware.
2. Fix recording pop noise on 3-byte audio firmware.

Version: 0.0.7

Change:

1. Send an input event to user space when detect OKG.
2. Fix kcontrol “HOTWORD Trigger” typo

Version: 0.0.6

Change:

1. Add time stamp ioctl and feature for loading module dynamically.

Version: 0.0.5

Change:

1. Modify copy work queue time

2. Mute dmic while doing time sync.

3. Add variable is\_spi\_ready to check whether spi resume.

Version: 0.0.4

Change:

1. Keep LED always lights up while recording.

Version: 0.0.3

Change:

1. Remain only one gpio for receiving IRQ instead of two gpio.

Version: 0.0.2

Change:

1. Add watchdog feature and dsp core reset control for watchdog self-test.
2. Add dsp idle mode control and soc time sync control.

Version: 0.0.1

Change:

1. Support time sync tick and system time and get the timestamp